Firmware auto update

Automatically initiate firmware update via HTTP with pointed URL (URL points custom.ini, section [system]) or via DHCP

Example:

Section content [system]

[system] update_url = 'http://<your_domain_or_ip>/update/'

On WEB-server in directory /update/ create directories /200 and/or /250 and place imageupdate there.

Admin interface

Firmware auto update (on)/(off) - opening and closing of a particular section of the automatic update

Add - adding sections to configure automatic updates. For example: there is a section for MAG200, you can add a separate section for MAG250 etc

STB-Model - STB model for which update is set

ImageVersion - ImageVersion number for updating (from image)

ImageDate - Image data (from image)

Required ImageDescription - Only STBs with Required ImageDescription will be updated.

Required ImageVersion - Only STBs with Required ImageVersion will be updated.

Update variant - http update (image update via HTTP), reboot dhcp (STB reboot in DHCP mode “boot mode - DHCP”)

<spoiler|Fig> </spoiler>