Specification STB MAG-200

Technical characteristics:

Display Modes:

HD 1080i
HD 720p
SD 576p/i
PAL/NTSC

Video Codecs:

MPEG1/2 MP@HL
H.264 HP@level 4.1
MPEG4 part 2 (ASP)
VC1 video,WMV-9 (optional)

Audio Codecs:

MPEG-1 layer I/II
MPEG-2 layer II
MPEG-2 layer III (mp3)\\ MPEG-2 AAC (опционально)
MPEG-4 AAC LC 2-ch/5.1ch (optional)
MPEG-4 AAC+SBR 2-ch/5.1ch (optional)
Dolby Digital (optional)

DVB subtitles
Stream media protocols: RTSP, RTP, UDP, IGMP

Overall dimensions MAXI:

300mm x 236mm x 65mm
Weight: 1700 g

Overall dimensions COMPACT:

240mm x 145mm x 45mm
Weigtt: 1500 g

Overall dimensions MINI:

170mm x 145mm x 45mm
Weight: 1300 g

hardware:

- STi7109/7101 processor. System-on-Chip (SoC)
- RAM DDR 128Mb
- ROM NOR Flash 1Mb, NAND Flash 128Mb
- Software power-off capable, 5 V; 2 A
- Power: 100~240 V, 50/60 Hz
- video out: RCA, S-Video, SCART, HDMI V1.3, Component RGB or (Y Pr Pb)
- audio out: S/PDIF (Dolby AC-3 multi-channel), LR RCA
- Ethernet 10/100TX Auto MDI/MDIX Base-T RJ-45
- USB 2.0
- IRDA RC-5 (36KHz)
- ETS 300-019-1-1 Class 3.1

Software

Fully compatible with MAG-100 (API JS, API C)
(Base Operating System linux2.6.16-18)
Internet agent: WebKit
built-in media portal functionality with IPTV
HTTP 1.1, HTML 4.01 XHTML 1.0/1.1
DOM 1, 2, 3, CSS 1, 2, 3
XML 1.0, XSLT 1.0, XPath 1.0
SOAP 1.1
JavaScript ECMA-262, revision 5
Media JavaScript API
C layer SDK