Configuring the media server (UPnP)

IPTV STB MAG-200 can play content from a media server (UPnP).

Enable UPnP client in the internal software STB MAG200/250

System settings (SETUP button on the RC).

Advanced settings.

UPnP client enabled: Off - UPnP client is off, LAN - UPnP is enabled on the LAN interface, Wireless - UPnP is enabled on the Wi-Fi interface.

UPnP Linux OS, Mac OS

For example: MediaTomb

UPnP Windows 7

For examle: TVersity

In the OS Microsoft Windows 7 contains built-in UPnP:

Enable UPnP Windows 7

Stream your media using Windows Media Player