How to flash the second image BootLoader MAG200/250?

Upgrade from USB-flash

Copy on a flash drive two files:

SbootIm
set_second_boot.sh

actual version set_second_boot.sh

Login to the STB via ssh

Login: root Password: 930920 Port: 22
Attention!!! Beginning from version 0.2.14-r8 the changes were implemented in security and update system. In manufacturer firmware version (firmware version, which is provided by manufacturer for Autoupdate and update from internal portal) - SSH is locked. In Public firmware versions, provided in http://soft.infomir.com.ua/mag250/release/ - SSH is open at standard port. Release description New instructions and utilities for firmware making

Connect the USB flash drive

Change into the directory in which files are copied earlier ( usually a flash drive is mounted in the directory /media/USB-…the device name.. ).

Run the command

set_second_boot.sh
*Reboot STB.

Update via http

Login to the STB via ssh

Run the commands

/bin/wget http://soft.infomir.com.ua/mag200/upgrade/Second_boot/set_second_boot.sh -O /ram/set_second_boot.sh
chmod a+x /ram/set_second_boot.sh
/ram/set_second_boot.sh http://soft.infomir.com.ua/mag200/upgrade/Second_boot/SbootIm

Reboot STB.

Probably as use of parameter for set_second_boot.sh In the form of

tftp://192.168.1.240/mag200/SbootIm

In this case the image of bootloader will be loaded by tftp protocol from a server with address 192.168.1.240 and name mag200/SbootIm. .