Flussonic DVR

Starting from v 4.9.11 flussonic support for TV archive was added in Stalker MW.

Timeshift from flussonic is supported starting from Stalker MW v4.9.19.

Configuration steps:

In Stalker MW Admin interface > Storages > Add new Storage, set IP of flussonic server and set flussonic port.

Select option Storing content, Record TV, Flussonic DVR.

Storage

In Stalker MW Admin interface > IPTV Channels > Channel > SET URL for recording in format http://FlussonicIP:port/<streamname>/index.m3u8 (for HLS)

Select options Enable TV Archive > Flussonic DVR > Storage that was previously created.

Set EPG for channel.

Channel

Enable DVR on flussonic

Flussonic

Flussonic Doc