Temporary URLs settings for Flussonic Media Server

Setup authorization on Flussonic side.

In Admin interface of Stalker MW > IPTV Channels > on channel enable next options Temporary HTTP URL and Flussonic support